


1. Open Devices -> Settings -> Device Role
2. Click on NEW…




1. Fill out Description = “BrocadeSwitch”
2. Select merge method “Merge on deice name with SNMP sysName, first”
3. Set checkbox “SNMP scan/walk allowed”
4. Confirm with OK



1. Go to “oid catalog”




1. Click on NEW…
2. Fill out
   1. ID=”1.3.6.1.4.1.1991.1.3.48.7.3”
   2. Description: ”Brocade-icx7750”
   3. Select merge method: “Merge on deice name with SNMP sysName, first”
   4. Object role: “BrocadeSwitch”
3. Confirm with OK



1. Import discovery files

**EXAMPLE:**



File with 9 port of one device icx7750-g3 were merged to one:

